HANGZHOU RUICHENG INSTRUMENT CO., LTD.

High-speed Mini-centrifuge—MC15K
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Introduction

The High-speed Mini-centrifuge is a compact centrifuge capable of achieving centrifugal speeds up to 15000rpm, that is approximately 15533g. It is used for extracting RNA/DNA samples, sedimentation of biological components, biochemical and chemical analysis of micro samples. Automatic imbalance switch-off and locking of lid provide safe operation. The rotor accepts 1.5 to 2.0ml tubes directly, as well as 0.5ml and 0.2ml tubes with optional adapters. 

Features:

LCD provides a clear indication of time and rpm or RCF. 

RPM/RCF setting as required.

The rotor is made of nylon material, with corrosion resistance, minimizes the temperature increases during longer run at high speed. 

Accelerates and decelerates in just 16seconds.

Safety operation: rotor imbalance diagnostic; automatic stop.

Motor overheating protection function.

A separate momentary short button permits instant spin downs. 

Low sample heating (only 5°C after 30min, at max. speed).

A brushless motor provides noiseless performance and long service life.

Parameters
	Model
	MC15K

	Capacity
	12x1.5/2.0ml centrifuge tubes

	Speed range
	500~15000rpm

	RCF range
	16~15533g

	Timing range
	15sec~99min59sec/∞

	Acceleration
	16sec(0~15000rpm)

	Deceleration
	16sec(15000~1000rpm)

	Rotor imbalance diagnostic
	Yes

	Motor overheating protection function
	Yes

	Power
	120W

	Voltage
	DC24V/5A

	Dimension(mm)
	255x194x140mm

	Weight
	2.3kg
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