Shaker for Microplates—MS300

[image: image1.jpg]



Description:
MS300 Shaker for Microplates is a high speed shaker with direct brushless DC motor and microprocessor controlled technique, specifically for elisa plate and cell culture plate. It can hold 2pcs elisa plates(96/384wells), deep-well plates and cell culture plates(24/48/96wells).
Features:

LCD real-time display system status and parameters.

Timer from 0 to 99h59min.

Support 2 standard microplates and deep well plates.
Brushless DC motor, low noise, small interference, free maintenance.
The built-in status indicator allows the user to quickly get the status of the device.

When timing ends, system will make an alarm voice automatically. 
Automatic fault detection and buzzer alarm function.
With special fixing way, install and disassemble the plates quickly, don’t need the additional tool.
Parameters:

	Time range
	1sec~99min59sec/1min ~ 99h59min/∞

	Speed range
	200～2000rpm

	Mixing orbit
	2mm

	Speed step value
	10rpm

	With status indicator light
	Yes

	Sample capacity
	2plates

	Power
	45W

	Voltage
	DC24V/2A

	Dimension(mm)
	294×200×107

	Weight(kg)
	3.8


Note: Please refer to the operation manual for the maximum speed of different kinds of plates.
