HANGZHOU RUICHENG INSTRUMENT CO., LTD.

Thermo Shaker—TS100, TSC10
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Description:

TS100/TCS10 Thermo Shaker is a temperature controlled shaker, which is useful for a variety of molecular biology applications. Speed, time and temperature settings are continuously visible on the LCD, simultaneously showing both actual and selected values. Integral over-temperature control ensures long time, safety and sample integrity.
Features:

LCD display. It is easy to setup and use.
Reliable design with inner extra temperature protection.

Each device is equipped with lifter that is easy to replace different blocks.

Digital accuracy and convenience.

Precision wells for uniform thermal transfer.

Assorted blocks for a wide variety of tube sizes.

Brushless DC Motor: noiseless long service life maintenance-free.

Conforms to CE safety standard.

Accurately control and display time, temperature and speed.
Applications:
Maintaining 14°C for ligation reactions.(TCS10)
Maintaining 17°C for storing oocytes.(TCS10)
Storing samples at ice bucket temperatures. (TCS10)
Storing enzymes or DNA libraries at your work station.
Transporting samples from the field at exactly the right temperature.

Heating samples in the field.
Enzyme reactions and deactivations.
PCR sample preparation.
Parameters:

	Model
	TS100
	TCS10

	Temp setting range
	0℃~100℃
	0℃~100℃

	Temp control range
	RT+5℃~100℃
	RT.-20℃~100℃

	Time range
	1min ~ 99h59min/∞
	1min ~ 99h59min/∞

	Temp accuracy
	≤±0.3℃
	≤±0.3℃

	Display accuracy
	0.1℃
	0.1℃

	Temp uniformity
	≤±0.3℃
	≤±0.3℃

	Speed range
	200~1800rpm
	200~1500rpm

	Orbit
	3mm
	3mm

	Heating time
	≤12min(from 25℃ to 100℃)
	≤12min(from 25℃ to 100℃)

	Cooling time1
	/
	≤10min(from 100℃ to 25℃)

	Cooling time2
	/
	≤15min(from RT. to RT.-20℃)

	Multi point running
	Yes(Max 5points)
	Yes(Max 5points)

	Multi cycle
	Yes(Max 99times)
）
	Yes(Max 99times)

	Auto heating
	Yes
	Yes

	Auto running
	Yes
	Yes

	Auto resume to run
	Yes
	Yes

	Storage at 4℃
	
	Yes

	Power supply
	150W
	150W

	Voltage
	AC220V or AC110V/50-60Hz
	AC110V~220V/50-60Hz

	Fuse
	250V 3A  Ф5×20
	250V 3A  Ф5×20

	Dimension(mm)
	260x195x150
	260x195x150

	Weight
	7.0kg
	7.5kg


	Type
	Description
	Max Speed (TS100)
	Max Speed (TCS10)

	MD30
	96x0.2ml
	1800rpm
	1500rpm

	MD31
	54x0.5ml
	1800rpm
	1500rpm

	MD32
	35x1.5ml
	1800rpm
	1500rpm

	MD33
	35x2.0ml
	1800rpm
	1500rpm

	MD34
	20x1.5ml+15x0.5ml
	1800rpm
	1500rpm

	MD35
	96x0.2ml
	1800rpm
	1500rpm

	MD36
	24x5ml
	1000rpm
	1000rpm

	MD37
	15x10ml
	1000rpm
	1000rpm

	MD38
	12x15ml
	800rpm
	800rpm

	MD39
	6x50ml

(round-shape bottom)
	800rpm
	800rpm

	MD39-S
	6x50ml

(cone-shape bottom)
	800rpm
	800rpm


Optional Blocks:
[image: image1.jpg]



Hangzhou Ruicheng Instrument Co., Ltd.

Add：Building E, No.8 of Houshan Road, Yuhang District, Hangzhou City, Zhejiang Province, China  

Tel：0571-88630940  Fax：0571-85126370

Email: info@ruiwell.com, sales2@ruiwell.com  Website: http://www.ruiwell.net

