HANGZHOU RUICHENG INSTRUMENT CO., LTD.

Orbital Shaker—MPS-10
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Description:
MPS-10 Orbital Shaker is a high speed shaker with direct brushless DC motor and microprocessor controlled technique. It can be applicable in different laboratories: in microbiology, biotechnology, medical analysis, etc.
Features:

· LCD displays time and shaking speed.

· Easy to operate with one-touch knob.

· Warm root and variety of platforms can be chosen.

· When time control ends, instrument will make alarm voice.

· Gentle and reliable shaking with direct brushless DC motor.

Parameters:

	           Type

Parameter
	MPS-10

	Time range
	1min~99h59min

	Speed range
	50～300rpm

	Orbit
	10mm

	Power
	50W

	Voltage
	AC100V~240V 50/60Hz

	Dimension(with PP-1)(mm)
	280×270×110

	Weight(with PP-1)(kg)
	7.0


Optional Platforms

	Type
	Description

	PP-1
	Flat platform for 8pcs petri dish

	PP-2
	Universal platform with adjustable bars, for 6x100ml or 4x250ml conical flask

	PP-3
	Platform with clamps for 12x100ml conical flask

	PP-3
	Platform with clamps for 6x250ml conical flask
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