HANGZHOU RUICHENG INSTRUMENT CO., LTD.

Sample Concentrator—ND100 series
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Description:

ND100 series sample concentrator is with microprocessor controlled and PID fuzzy controlled technique. Instead of traditional water bath device, the heat-conducting medium is high purity aluminum. The test tubes are held in a block, and blowing a large number of samples at one time.

It can used in residue analysis, commodity inspection, food, environment, pharmacy and biological product and other industries.
Features:
High precision and wide range of temp control.

Blowing a large number of samples at a time.

Blowing each sample independently.

Amount of airflow can be adjusted.

Easy operation; safe and reliable to use.

Parameters:

	Model
	ND100-1
	ND100-2

	Temp range
	RT.+5℃ -160℃
	RT.+5(C -160(C

	Temp accuracy
	±0.5℃(@40℃)
	±0.5℃(@40℃)

	Temp accuracy
	±1℃(@120℃)
	±1℃(@120℃)

	Temp uniformity
	±0.5℃
	±0.5℃

	Display accuracy
	0.1℃
	0.1℃

	Timing range
	1min-99h59min/∞
	1min-99h59min/∞

	Heating time
	≤15min(from 25℃ to 160℃)
	≤15min(from 25℃ to 160℃)

	Max vertical travel
	200mm
	200mm

	Nitrogen flow rate
	15L/min
	15L/min

	Nitrogen pressure
	0.02Mpa(Gas needle≤16pcs)
0.05Mpa(Gas needle＞16pcs)
	0.02Mpa(Gas needle≤16pcs)
0.05Mpa(Gas needle＞16pcs)

	Block quantity
	1
	2

	Power
	300W
	500W

	Voltage
	AC220V or AC110V, 50/60Hz
	AC220V or AC110V, 50/60Hz

	Dimension(mm)
	260x20x50
	260x220x450

	Weight(kg)
	7.0
	7.5


Optional Blocks:
	Type
	Description
	Type
	Description

	MD03
	24x10mm
	MD09
	12x20mm

	MD04
	24x12mm
	MD10
	8x26mm

	MD05
	24x13mm
	MD11
	4x28mm

	MD06
	16x15mm
	MD12
	3x40mm

	MD07
	16x16mm
	MD15
	24x1.5ml(centrifuge tube)

	MD08
	12x19mm
	MD16
	24x2.0ml(centrifuge tube)
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Hangzhou Ruicheng Instrument Co., Ltd.

Add：Building E, No.8 of Houshan Road, Yuhang District, Hangzhou City, Zhejiang Province, China  

Tel：0571-88630940  Fax：0571-85126370

Email: info@ruiwell.com, sales2@ruiwell.com  Website: http://www.ruiwell.net

