Thermo Shaker for Microplates—TS200
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Description:
TS200 Thermo Shaker for Microplates is with technique of brushless DC motor and PID intelligent temperature control. Mainly used for shaking and cultivation in elisa plates (96/384 wells) or 96 wells tissue culture plates.

Features:

LCD displays system status and parameters.

Stable and reliable operation with high quality switch.

Easy to operate with one touch knob.

Set-up the time within 0~100hours, instrument will make alarm voice when completing.

With power recovery, instrument will be continuous to run when power recovers from outage.

Applications:
Storing enzymes or DNA libraries at your workstation.
Transporting samples from the field at exactly the right temperature.

Heating samples in the field.
Enzyme reactions and deactivations.
PCR sample preparation.
	Type

Parameter
	TS200

	Temp. range
	RT.+5℃ ~80℃

	Timing range
	1min ~ 99h59min

	Speed range
	200 ~ 1600rpm

	Orbit
	3mm

	Temp. Accuracy
	≤±0.5℃

	Display Accuracy
	0.1℃

	Temp. Uniformity
	≤±0.5℃

	Heating time
	≤10min(from RT. to 80℃)

	Sample capacity
	2pcs microplates or culture plates

	Heating part
	Heating film

	Power
	150W

	Voltage
	AC220V or 110V/50~60Hz

	Dimension(mm)
	280×270×140

	Weight(kg)
	7.0


