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TSM100 Thermal Shaking Unit
TSM100 Thermal Shaking Unit integrates mixing and heating functions, with speed of 300~2000 rpm and temperature control range RT.+ 5℃~110℃. It operates smoothly with low noise and provides excellent mixing performance. It features an automatic clamping function and a central origin selfpositioning function, making it compatible with other precision motion automation equipment. 

Features: 
1. The device features an automatic clamping function, which can automatically clamp and release plates or adapters, making it easy for robotic arms to pick up microplates and ensuring the safety and stability of adapters during high-speed shaking. 
2. The device features central origin self-positioning function, working with robotic arms to precisely clamp plates and pipettes for accurate liquid handling. 
3. [bookmark: _GoBack]The device integrates mixing and heating functions, simultaneous shaking and heating, or just heating or just shaking.
Basic parameters：

	Project
	Parameter

	Temp. setting range
	0℃~ 110℃

	Temp. control range
	RT.+5℃~ 110℃  

	Temp. accuracy 
	≤±0.3℃  

	Display accuracy 
	0.1℃

	Temp. uniformity
	≤±0.5℃ 

	Speed range
	300~2000rpm

	Orbit
	2mm

	Power
	120W

	Voltage
	DC24V

	[bookmark: OLE_LINK4][bookmark: OLE_LINK5]Communication interface
	485

	Dimension
	160x115x93mm

	Weight
	2.5kg
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