HANGZHOU RUICHENG INSTRUMENT CO., LTD.

Overhead stirrer VS20, VS40, VS70
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Description:

Overhead stirrer features stepless speed control and a DC brushless motor, with digital display of operating speed. It is characterized by constant speed and automatic torque adjustment. Its automatic overload and abnormal condition protection to ensure efficient and safe experiments. It is suitable for mixing low to high viscosity liquids or solid-liquid mixtures, and isdely used in chemical synthesis, pharmaceuticals, physicochemical analysis, and other fields.

Features:

Colorful LCD(320x240 Pixel) displays speed, time and status.
Stirring paddle “through-shaft” design, easy to adjust impeller position and  
replace the container.
Multiple protection: automatically shut down and alarm in the event of overload, short circuit, over-temperature, abnormal speed, etc. 

Brushless DC motor, low noise, small interference, free maintenance.
Self - locking drill chuck, tools free.
Set speed can be maintained when viscosity of liquid changes. 

Directly connect to computer via USB interface for remote control and 

speed recording.

Parameters:

	Model
	VS20
	VS40
	VS70

	Speed range
	30~2500rpm
	30~2500rpm
	30~1600rpm

	Speed control accuracy
	±1rpm
	±1rpm
	±1rpm

	Timing range
	0~ 99h59min
	0~ 99h59min
	0~ 99h59min

	Max. torque
	40N.cm
	60N.cm
	100N.cm

	Max. stirring volume(H2O)
	20L
	40L
	70L

	Max. viscosity 
	10000mPa.s
	50000mPa.s
	100000mPa.s

	Chuck clamp diameter range 
	0.5~10mm
	0.5~10mm
	0.5~10mm

	Communication interface
	USB(1 port)
	USB(1 port)
	USB(1 port)

	Overload protection
	Yes
	Yes
	Yes

	Power
	120W
	180W
	180W

	Voltage
	DC24V
	DC24V
	DC24V

	Dimension(mm)
	200x827x481
	200x827x481
	 200x827x481

	Weight(kg)
	8.3
	8.4
	8.6


Optional stirring tools
	Model
	Name
	Dimension

(mm×mm)
	Max. Speed

(rpm)
	Remark
	Picture

	RC02107001
	Propeller stirrer 
	400×50
	2500
	Standard stirring, applications at medium and high speed.
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	RC02107002
	Straight stirrer 
	400×60
	2500
	For low viscosity media at medium and high speeds
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	RC02107003
	Paddle stirrer 
	400×68
	1200
	For gentle mixing at low and medium speeds
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	RC02107004
	Centrifugal stirrer
	400×90
	2500
	Blades open while speeding. For narrow neck vessels at medium to high speed.
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	RC02107005
	Grand propeller stirrer 
	600×100
	2500
	Standard stirring
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	RC02107006
	Grand paddle stirrer 
	600×100
	500
	Gentle mixing for those stratify easily or sensitive to shear
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	RC02107007
	Grand anchor stirrer 
	600×100
	500
	Standard stirring for those easily precipitate
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	RC02107008
	Grand dissolving stirrer
	600×100
	2500
	Breaking down granules in the mixture with strong shear
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	RC02107009
	Flat-blade stirrer 
	400×60
	2500
	Suitable for medium speed stirring, low viscosity and medium viscosity materials
	[image: image10.jpg]




	RC02107010
	Anchor stirrer 
	400×60
	1200
	Suitable for low speed stirring, medium viscosity and high viscosity materials
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	RC02107011
	Spiral stirrer   
	350×50
	2500
	Suitable for medium speed or high speed agitation, medium viscosity and high viscosity materials, recommended for liquid homogenization or suspension treatment
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	RC02107012
	Radial-flow stirrer 
	400×50
	2500
	Suitable for medium speed or high speed agitation,  low viscosity and medium  viscosity materials, recommended for the treatment of gas in liquid
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Before operation, please
check the position of
stirrer and sample,





Hangzhou Ruicheng Instrument Co., Ltd.

Add：Building E, No.8 of Houshan Road, Yuhang District, Hangzhou City, Zhejiang Province, China  

Email: info@ruiwell.com, sales2@ruiwell.com  Website: http://www.ruiwell.net

