Shaker for Microplates—MS100
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Description:
MS100 Shaker for Microplates is a type of high speed shaker, which is with brushless DC motor and microprocessor controlled technique, specially for elisa plates (96/384 wells), tissue culture plates (24/48/96 wells).

Features:

LCD display system status and parameters. 

Stable and reliable shaking.

Easy to operate with one touch knob.

Automatic fault detection and buzzer alarm function.

Parameters:

	        Type

Parameter 
	MS100

	Time range
	1min~99h59min

	Speed range
	200~1500rpm

	Mixing orbit
	3mm

	Speed step value
	10rpm

	Sample capacity
	4plates

	Power
	45W

	Voltage
	AC100V~240V 50/60Hz

	Dimension(mm)
	280×270×140

	Weight(kg)
	4.0


